**Highlights**

* It combines DCNN classification network with image processing algorithms.
* It first uses RPCA to restore the sparse defects of STM images.
* It uses unique self-positioning method in the image processing.